FLOW RATE TO 850 LPM(224.5 GPM)(51 M³/ Hr. )(Pressure Ratio – 1 : 1) AIR SUPPLY PRESSURE = 2 BAR (29.01 PSIG) to 8.6 BAR (124.7 PSIG) Port Size –Tri - Clamp / Bolted Connections (Optional) Liquid Inlet / Suction Port – 3" Liquid Outlet / Discharge Port - 3" Air Inlet – ¾" (19mm) BSP Air Exhaust - 1" Female NPT (Includes Neo-Muff Silencer) | Note: Pump incorporated with Neo-Tef PTFE Diaphragms will reduce the Output by 28% Flow Rate: 610 LPM (161 GPM) (36.6 M3/Hr.) | | | | | | | | | | | | | | | | | | | | | | | | | EOM sf 75 EOM Flammable Product Transfer Safety Manual BROCHURE sf 75 Brochure FLYERS Neo-Flo Design Saniflux Flyer Neo-Flo Competitive Matrix SPARES LIST sf 75 Spares List
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Suction Lift Rubber Diaphragm PTFE Diaphragms Dry – 4.1 meter (13.4 ft.) Dry – 3.0 meter (9.84 ft.) Wet – 8.5 meter (27.9 ft.) Wet – 8.2 meter (27.9 ft.) - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - |
Maximum Particle Size / Maximum Compressible Solids: Ball Valve - ¾" (19.1 mm) , Flap Valve - 2-½" (63.5 mm) Displacement per Stroke* – 1.09 Liter (0.28 gallon) Ship Weight Stainless Steel 316 ………… 99kg. (219 lb.) Typical Noise Level - 69dB (with Neo-Muff Silencer) Pump Dimensions – Height 1225mm (48") X Width 642mm (25") X Depth 432mm (17") * Displacement per stroke was calculated at 4.9 bar (71 psig) air inlet pressure against a 2.2 bar (31 psig) head pressure.