FLOW RATE TO 210 LPM (55 GPM) (12.6 M³ / Hr.) (Pressure Ratio – 1 : 1) AIR SUPPLY PRESSURE = 2 BAR (29.01 PSIG) to 8.6 BAR (124.7 PSIG) Port Size – ANSI Flange Liquid Inlet / Suction Side – 1" Liquid Outlet / Discharge Side - 1" Air Inlet – ½" BSP Air Exhaust - ½" Female NPT (Includes Neo-Muff Silencer). | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | EOM nfp 25 EOM Flammable Product Transfer Safety Manual BROCHURE nfp 25 Brochure FLYERS Neo-Flo Design Neo-Flo Competitive Matrix SPARES LIST nfp 25 Spares List
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Suction Lift Rubber Diaphragm PTFE Diaphragm Dry - 3.4 meter (11.8 ft.) Dry – 2.2 meter (7.2 ft.) Wet – 9.0 meter (29.5 ft.) Wet – 8.8 meter (28.8 ft.) - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - |
Maximum Particle Size / Maximum Solids Passage – 3/16" (5.1mm) Displacement per Stroke* – 0.30 Liter (0.08 gallon) Typical Noise Level - 70dB (with Neo-Muff Silencer) Ship Weight Polypropylene ……………….…… 15 kg. (33 lb.) Pump Dimensions – Height 437mm (17.2") X Width 468mm (18.4") X Depth 257mm (10.1") * Displacement per stroke was calculated at 4.9 bar (71 psig) air inlet pressure against a 2.2 bar (31 psig) head pressure. - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Performance Chart - - - - - - - - - - - - - - - - - - Flow indicates in chart are determined by pumping water. Based on Specific Gravity of 1.0 For optimum life and performance, pumps should be specified so that daily operation parameters will fall in the center of the pump performance curve.