FLOW RATE TO 1009LPM(267GPM)(60.5M³/Hr.)(Pressure Ratio - 1:1) AIR SUPPLY PRESSURE = 2BAR(29.01 PSIG) to 8.6BAR(124.7 PSIG) Port Size – DIN OR ANSI Combo Flange (180° Rotational) Liquid Inlet / Suction Side – 3" Liquid Outlet / Discharge Side - 3" Air Inlet – ¾" BSP Air Exhaust - 1" Female NPT (Includes Neo-Muff Silencer). | Note: Pump incorporated with Neo-Tef PTFE Diaphragms will reduce the Output by 26% Flow Rate: 740 LPM (196 GPM) (44.4 M3/Hr.) | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | EOM nf 75 (Aluminum) EOM nf 75 (SS-304) EOM Flammable Product Transfer Safety Manual BROCHURE nf 75 Brochure FLYERS Neo-Flo Design Neo-Flo Competitive Matrix SPARES LIST nf 75 Spares List
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Suction Lift Rubber Diaphragm PTFE Diaphragm Dry – 6.0 meter (19.7 ft.) Dry – 4.1 meter (13.4 ft.) Wet – 8.4 meter (27.6 ft.) Wet – 7.4 meter (24.2 ft.) - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - |
Maximum Solids Passage/ Maximum Compressible Solids –1/2" (12.7mm) Displacement per Stroke* – 5.13 Liter (1.35 gallon) Typical Noise Level - 69dB (with Neo-Muff Silencer) Ship Weight Aluminum ……………….…… 90 kg. (198.4 lb.) SS - 304 ……………….…… 140 kg. (309 lb.) Pump Dimensions – Height 1050mm (41") X Width 630mm (25") X Depth 430mm (17") * Displacement per stroke was calculated at 4.9 bar (71 psig) air inlet pressure against a 2.2 bar (31 psig) head pressure. - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Performance Chart - - - - - - - - - - - - - - - - - - - Flow indicates in chart are determined by pumping water. Based on Specific Gravity of 1.0 For optimum life and performance, pumps should be specified so that daily operation parameters will fall in the center of the pump performance curve.