Output indicates in chart are determined by pumping water. Based on Specific Gravity of 1.0 For optimum life and performance, pumps should be specified so that daily operation parameters will fall in the center of the pump performance bar. | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - | - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - FLOW RATE UPTO 112 LPM (29.5 GPM) (6.72 M³ / Hr.) AIR SUPPLY PRESSURE = 2 BAR (29.01 PSIG) to 3.4 BAR (50 PSIG) MAX. Port Size – DIN OR ANSI Flange Liquid Inlet / Suction Side – 1" Liquid Outlet / Discharge Side - 1" Air Inlet – ½" BSP Air Exhaust ½" Female NPT (Includes Neo-Muff Silencer) Maximum Particle Size / Maximum Solids Passage – 1/8" (3.2mm) Displacement per Stroke* – 0.30 Liter (0.08 gallon) Typical Noise Level – 66 dba @ 3.1 bar (45 p.s.i) Air Pressure Dynamic Viscosity upto 25,000 Centipoise More Specs
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - | - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - FLOW RATE UPTO 290 LPM (76.6 GPM) (17.4 M³ / Hr.) AIR SUPPLY PRESSURE = 2 BAR (29.01 PSIG) to 3.4 BAR (50 PSIG) MAX. Port Size – DIN OR ANSI Flange Liquid Inlet / Suction Side – 2" Liquid Outlet / Discharge Side - 2" Air Inlet – ¾" BSP Air Exhaust - 1" Female NPT (Includes Neo-Muff Silencer) Maximum Particle Size / Maximum Solids Passage –1/4" (6.5mm) Displacement per Stroke* – 3.0 Liter (0.79 gallon) Typical Noise Level – 69 dba @ 3.1 bar (45 p.s.i) Air Pressure Dynamic Viscosity upto 55,000 Centipoise More Specs
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - | - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - FLOW RATE UPTO 461 LPM (121.7 GPM) (27.7 M³ / Hr.) AIR SUPPLY PRESSURE = 2 BAR (29.01 PSIG) to 3.4 BAR (50 PSIG) MAX. Port Size – DIN OR ANSI Flange (360° Rotational) Liquid Inlet / Suction Side – 3" Liquid Outlet / Discharge Side - 3" Air Inlet – ¾" BSP Air Exhaust - 1" Female NPT (Includes Neo-Muff Silencer) Maximum Particle Size / Maximum Solids Passage –1/2" (12.5mm) Displacement per Stroke* – 5.10 Liter (1.35 gallon) Typical Noise Level – 69 dba at 3.1 bar (45 p.s.i) Air Pressure Dynamic Viscosity upto 80,000 Centipoise More Specs