FLOW RATE TO 135 LPM(35.6 GPM)(8.10 M³ / Hr.)(PressureRatio – 1 : 1) AIR SUPPLY PRESSURE = 2 BAR(29.01 PSIG) to 8.6 BAR(124.7 PSIG) Port Size –Tri - Clamp Connections Liquid Inlet / Suction Port – 1" Liquid Outlet / Discharge Port - 1" Air Inlet – ½" BSP Air Exhaust - ½" Female NPT (Includes Neo-Muff Silencer) | Note: Pump incorporated with Neo-Tef PTFE Diaphragms will reduce the Output by 19% Flow Rate: 110 LPM (29.1 GPM) (6.6 M3/Hr.) | | | | | | | | | | | | | | | | | | | | | | | | | | EOM sf 25 EOM Flammable Product Transfer Safety Manual BROCHURE sf 25 Brochure FLYERS Neo-Flo Design Saniflux Flyer Neo-Flo Competitive Matrix SPARES LIST sf 25 Spares List
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Suction Lift Rubber Diaphragm PTFE Diaphragms Dry - 3.3 meter (10.8 ft.) Dry – 2.0 meter (6.5 ft.) Wet - 8.3 meter (27.2 ft.) Wet – 8.1 meter (26.5 ft.) - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - |
Maximum Particle Size / Maximum Compressible Solids: Ball Valve - 5.5mm Displacement per Stroke* – 0.3 Liter (0.07 gallon) (Rubber Fitted) , 0.05 Liter (0.02 Gallon) (PTFE Fitted) Ship Weight Stainless Steel 316 ………… 50 kg. (110 lb.) Typical Noise Level - 69dB (with Neo-Muff Silencer) Pump Dimensions – Height 1010mm (40") X Width 472mm (19") X Depth 400mm (16") * Displacement per stroke was calculated at 4.9 bar (71 psig) air inlet pressure against a 2.2 bar (31 psig) head pressure.