Output indicates in chart are determined by pumping water. Based on Specific Gravity of 1.0 For optimum life and performance, pumps should be specified so that daily operation parameters will fall in the center of the pump performance bar. | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - | - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - FLOW RATE UPTO 151 LPM (39.9 GPM) (9.06 M³ / Hr.) AIR SUPPLY PRESSURE = 2 BAR (29.01 PSIG) to 8.6 BAR (124.7 PSIG) Port Size –Tri - Clamp Connections Liquid Inlet / Suction Port – 1" Liquid Outlet / Discharge Port - 1" Air Inlet – ½" BSP Air Exhaust ½" Female NPT (Includes Sanitary Neo-Muff Silencer) Maximum Particle Size / Maximum Solids Passage – ¼" (6.2mm) Displacement per Stroke* – 0.32 Liter (0.08 gallon) Typical Noise Level – 65 dba at 3.5 bar Air Pressure Dynamic Viscosity upto 25,000 Centipoise More Specs
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - | - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - FLOW RATE UPTO 581 LPM (153.5 GPM) (34.86 M³ / Hr.) AIR SUPPLY PRESSURE = 2 BAR (29.01 PSIG) to 8.6 BAR (124.7 PSIG) Port Size –Tri - Clamp Connections Liquid Inlet / Suction Port – 2" Liquid Outlet / Discharge Port - 2" Air Inlet – ¾" BSP Air Exhaust - 1" Female NPT (Includes Sanitary Neo-Muff Silencer) Maximum Particle Size / Maximum Solids Passage –½" (12.7mm) Displacement per Stroke* – 1.09 Liter (0.28 gallon) Typical Noise Level – 65 dba at 3.5 bar Air Pressure Dynamic Viscosity upto 55,000 Centipoise More Specs
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - | - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - FLOW RATE UPTO 850 LPM (224.5 GPM) (51 M³ / Hr. ) AIR SUPPLY PRESSURE = 2 BAR (29.01 PSIG) to 8.6 BAR (124.7 PSIG) Port Size –Tri - Clamp Connections Liquid Inlet / Suction Port – 3" Liquid Outlet / Discharge Port - 3" Air Inlet – ¾" BSP Air Exhaust - 1"Female NPT (Includes Sanitary Neo-Muff Silencer) Maximum Particle Size / Maximum Solids Passage –¾" (19.1 mm) Displacement per Stroke* – 2.79 Liter (0.74 gallon) Typical Noise Level – 69 dba at 3.5 bar Air Pressure Dynamic Viscosity upto 80,000 Centipoise More Specs