Type = Sealless Configuration = Horizontal FLOW RATE = 483 LPM (128 GPM) (29 M3 / Hr.) MAX. OPERATING TEMPERATURE = 79°C (175°F) MAX. WORKING PRESSURE = 6 BAR (87 PSIG) MAX. HEAD = 26 METERS (85.3 FT.) MAX. Viscosity = 150 Centipoise (1.5 Poise) MAX. Specific Gravity = 1.8 Port Size – ANSI / DIN Flange Liquid Inlet / Suction Side – 2" (51mm) Liquid Outlet / Discharge Side - 1½" (38mm) - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Wetted Path : Volute & Casing Glass Fiber Reinforced Polypropylene (GFRPP) Poly Vinyl Di Fluoride (PVDF) - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Bearing Kit : Bearing / Shaft / Thrust Rings Carbon (Please refer Bearing Kit Options) - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Impeller Type : (G2.5 Balanced) Closed-ended Impeller (MOC – GFRPP) - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - O-rings : Viton (Please refer O-ring Options) - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Fasteners : Stainless Steel – 304 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Motor Ratings : (Please refer Motor Options) 3HP (2.2 kW) 2900RPM @ 50Hz. Efficiency = Three Phase – 415 Volt Ampere = - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Rated Point : 248 lpm (65.5 gpm) @ 2.5 Bar (36 psig) - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Maximum Particle Size : Slurries - 100µ (Microns) In-frequent Particles – 0.4mm - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - | Magnetic Capsule : Inner Drive Magnet Neodymium Iron Boron Magnets Encapsulated in Unfilled Polypropylene (NdFeB) Outer Drive Magnet Nickel-Plated Neodymium Iron Boron Magnets / Steel Note : Pump incorporated with Teflon Gasket has Max. Working Pressure of 3.5 BAR (50 psig)
Size | 50Hz. (2900 RPM) Impeller Dia. | 60Hz. (3450 RPM) Impeller Dia.
1 | 5.75” (146mm) | -
2 | 5.50” (140mm) | -
3 | 5.25” (133mm) | -
4 | 5.00" (127mm) | -
5 | - | 5.13" (130mm)
6 | - | 5.00” (127mm)
7 | - | 4.75” (116mm)
8 | - | 4.50” (114mm)
9 | - | 4.25” (108mm)
NOTE : Select Impeller from Performance Curve NOTE : Standard orders are shipped with impellers that have not been trimmed and are at maximum size. NOTE : All impeller diameters shown in “mm” size & are variable in one (1) millimeter increments. NOTE : Orders for units with trimmed impeller will be changed out at the factory before shipment. | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | EOM NMP3H EOM BROCHURE NMP3H Brochure FLYERS Neo-Mag Design SPARES LIST NMP3H Spares List
Maximum Hardness : 80 HS - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Maximum Concentration : 10% by Weight - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Ship Weight: GFRPP ……………. 48Kgs. (105.8 lbs.) - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Pump Dimensions: Length 570mm X Breath 305mm X height 280mm - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - NMP2H Performance Graph (2900RPM) - - - - - - - - - - - - - - - - - Note: Gravity-feed, Requires the Pump Inlet to be lower than Liquid Level Centrifugal Pump Impeller Rule of Thumb !!! Bigger the Impeller Diameter, Higher the Motor HP Consumption Bigger the Impeller Diameter, Higher the Output Bigger the Impeller Diameter, Higher the Discharge Pressure / Head Flow indicates in chart are determined by pumping water at sea level. Based on Specific Gravity of 1.0, ambient temperature 20°C (68°F). For optimum life and performance, pumps should be specified so that daily operation parameters will fall in the center of the pump performance curve.