FLOW RATE TO 581 LPM(153.5 GPM)(34.86 M³/Hr.)(Pressure Ratio – 1 : 1) AIR SUPPLY PRESSURE = 2 BAR (29.01 PSIG) to 8.6 BAR (124.7 PSIG) Port Size – Tri - Clamp Connections Liquid Inlet / Suction Port – 2" Liquid Outlet / Discharge Port - 2" Air Inlet – ¾" BSP Air Exhaust - 1" Female NPT (Includes Neo-Muff Silencer) | Note: Pump incorporated with Neo-Tef PTFE Diaphragms will reduce the Output by 37% Flow Rate: 361 LPM (95.4 GPM) (21.7 M3/Hr.) | | | | | | | | | | | | | | | | | | | | | | | | | | EOM sf 50 EOM Flammable Product Transfer Safety Manual BROCHURE sf 50 Brochure FLYERS Neo-Flo Design Saniflux Flyer Neo-Flo Competitive Matrix - pdf SPARES LIST sf 50 Spares List
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Suction Lift Rubber Diaphragm PTFE Diaphragms Dry – 3.2 meter (10.5 ft.) Dry – 2.4 meter (7.87 ft.) Wet – 9.0 meter (29.5 ft.) Wet – 8.7 meter (28.5 ft.) - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - |
Maximum Particle Size / Maximum Compressible Solids: Ball Valve - ½" (12.7mm) , Flap Valve - 1-5/8" (41.5 mm) Displacement per Stroke* – 1.09 Liter (0.28 gallon) Ship Weight Stainless Steel 316 ………… 50 kg. (110 lb.) Typical Noise Level - 69dB (with Neo-Muff Silencer) Pump Dimensions – Height 1010mm (40") X Width 472mm (19") X Depth 400mm (16") * Displacement per stroke was calculated at 4.9 bar (71 psig) air inlet pressure against a 2.2 bar (31 psig) head pressure.