FLOW RATE TO 675 LPM(178 GPM)(40.5 M³ / Hr.)(Pressure Ratio – 1 : 1) AIR SUPPLY PRESSURE = 2 BAR (29.01 PSIG) to 8.6 BAR (124.7 PSIG) Port Size – DIN OR ANSI Combo Flange Liquid Inlet / Suction Side – 2" Liquid Outlet / Discharge Side - 2" Air Inlet – ¾" BSP Air Exhaust - 1" Female NPT (Includes Neo-Muff Silencer). | Note: Pump incorporated with Neo-Tef PTFE Diaphragms will reduce the Output by 20% Flow Rate: 540 LPM (143 GPM) (32.4 M3 / Hr.) | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | EOM nf 50 EOM Flammable Product Transfer Safety Manual BROCHURE nf 50 Brochure FLYERS Neo-Flo Design Neo-Flo Competitive Matrix SPARES LIST nf 50 Spares List
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Suction Lift Rubber Diaphragm PTFE Diaphragm Dry – 7.0 meter (23 ft.) Dry – 4.0 meter (13.1 ft.) Wet – 9.0 meter (29.5 ft.) Wet – 8.3 meter (27.2 ft.) - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - |
Maximum Solids Passage/ Maximum Compressible Solids Passage –1/4" (6.5mm) Displacement per Stroke* – 3.0 Liter (0.79 gallon) Typical Noise Level - 69dB (with Neo-Muff Silencer) Ship Weight Aluminum ……………….…… 43 kg. (94 lb.) Pump Dimensions – Height 762mm (30") X Width 441mm (17.4") X Depth 381mm (15") * Displacement per stroke was calculated at 4.9 bar (71 psig) air inlet pressure against a 2.2 bar (31 psig) head pressure. - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - Performance Chart - - - - - - - - - - - - - - - - - - - Flow indicates in chart are determined by pumping water. Based on Specific Gravity of 1.0 For optimum life and performance, pumps should be specified so that daily operation parameters will fall in the center of the pump performance curve.