WELCOME ! Neoflux understands that a complex design or solution does not necessarily breed success. Our product ranges are designed to exceed industry standards cost effectively and efficiently. The more intuitive the product or solution is, the easier your specification, operation and maintenance becomes. If you are looking for a single pump that can be used in a wide variety of applications, you want Air-Operated Double Diaphragm Pump (AODDP) from Neoflux. We provide the most complete line of AODD Pumps available, as well as full selection of diaphragm & accessories. The Neoflux Air-Operated Double Diaphragm Pump is available in various sizes ranging from 1" to 4" allowing for optimum flow rates. A wide variety of construction options are available to meet virtually any application requirement. The Neoflux pump can handle pressures up to 8.6 bar (125 psig) and temperatures to 176.7° C (350° F). Liquid path materials of construction include: Aluminum, Stainless Steel & Polypropylene. | | | | | | | | | | | | | | | | | | | |
Ease of Specification Neoflux is staffed with quality pump professionals and a 20-year knowledge base. Our literature is comprehensive with state-of-the-art support and validation materials. Ease of Operation Our design simplicity fosters ease of operation. The flow rate and pressure is adjusted by simply adjusting air pressure, air volume and / or discharge head. Troubleshooting system problems is easy due to the low number of moving parts and simplicity and durability of the Neo-Flo design. Ease of Maintenance Neoflux has refined its technology over the past 10 years. We have made technological advancements to enhance the pump's reliability without sacrificing the ease of maintenance. The lowest parts-per-pump in the industry assure that your maintenance programs result in low direct maintenance expenses and down-time. | How AODD Pump Works?